Overview
--------
- BSC9131 is integrated device that targets Femto base station market.
 It combines Power Architecture e500v2 and DSP StarCore SC3850 core
 technologies with MAPLE-B2F baseband acceleration processing elements.
- It's MAPLE disabled personality is called 9231.

The BSC9131 SoC includes the following function and features:
. Power Architecture subsystem including a e500 processor with 256-Kbyte shared
  L2 cache
. StarCore SC3850 DSP subsystem with a 512-Kbyte private L2 cache
. The Multi Accelerator Platform Engine for Femto BaseStation Baseband
  Processing (MAPLE-B2F)
. A multi-standard baseband algorithm accelerator for Channel Decoding/Encoding,
 Fourier Transforms, UMTS chip rate processing, LTE UP/DL Channel processing,
 and CRC algorithms
. Consists of accelerators for Convolution, Filtering, Turbo Encoding,
 Turbo Decoding, Viterbi decoding, Chiprate processing, and Matrix Inversion
 operations
. DDR3/3L memory interface with 32-bit data width without ECC and 16-bit with
 ECC, up to 400-MHz clock/800 MHz data rate
. Dedicated security engine featuring trusted boot
. DMA controller
. OCNDMA with four bidirectional channels
. Interfaces
. Two triple-speed Gigabit Ethernet controllers featuring network acceleration
  including IEEE 1588. v2 hardware support and virtualization (eTSEC)
. eTSEC 1 supports RGMII/RMII
. eTSEC 2 supports RGMII
. High-speed USB 2.0 host and device controller with ULPI interface
. Enhanced secure digital (SD/MMC) host controller (eSDHC)
. Antenna interface controller (AIC), supporting three industry standard
  JESD207/three custom ADI RF interfaces (two dual port and one single port)
  and three MAXIM's MaxPHY serial interfaces
. ADI lanes support both full duplex FDD support and half duplex TDD support
. Universal Subscriber Identity Module (USIM) interface that facilitates
  communication to SIM cards or Eurochip pre-paid phone cards
. TDM with one TDM port
. Two DUART, four eSPI, and two I2C controllers
. Integrated Flash memory controller (IFC)
. TDM with 256 channels
. GPIO
. Sixteen 32-bit timers

The e500 core subsystem within the Power Architecture consists of the following:
. 32-Kbyte L1 instruction cache
. 32-Kbyte L1 data cache
. 256-Kbyte L2 cache/L2 memory/L2 stash
. programmable interrupt controller (PIC)
. Debug support
. Timers

The SC3850 core subsystem consists of the following:
. 32 Kbyte 8-way level 1 instruction cache (L1 ICache)
. 32 Kbyte 8-way level 1 data cache (L1 DCache)
. 512 Kbyte 8-way level 2 unified instruction/data cache (M2 memory)
. Memory management unit (MMU)
. Enhanced programmable interrupt controller (EPIC)
. Debug and profiling unit (DPU)
. Two 32-bit timers

BSC9131RDB board Overview
-------------------------
 1Gbyte DDR3 (on board DDR)
 128Mbyte 2K page size NAND Flash
 256 Kbit M24256 I2C EEPROM
 128 Mbit SPI Flash memory
 USB-ULPI
 eTSEC1: Connected to RGMII PHY
 eTSEC2: Connected to RGMII PHY
 DUART interface: supports one UARTs up to 115200 bps for console display
 USIM connector

Frequency Combinations Supported
--------------------------------
Core MHz/CCB MHz/DDR(MT/s)
1. 1000/500/800
2. 800/400/667

Boot Methods Supported
-----------------------
1. NAND Flash
2. SPI Flash

Default Boot Method
--------------------
NAND boot

Building U-boot
--------------
To build the u-boot for BSC9131RDB:
1. NAND Flash
	make BSC9131RDB_NAND
2. SPI Flash
	make BSC9131RDB_SPIFLASH

Memory map
-----------
 0x0000_0000	0x7FFF_FFFF	DDR			1G cacheable
 0xA0000000	0xBFFFFFFF	Shared DSP core L2/M2 space	512M
 0xC100_0000	0xC13F_FFFF	MAPLE-2F		4M
 0xC1F0_0000	0xC1F3_FFFF	PA SRAM Region 0	256K
 0xC1F8_0000	0xC1F9_FFFF	PA SRAM Region 1	128K
 0xFED0_0000	0xFED0_3FFF	SEC Secured RAM		16K
 0xFEE0_0000	0xFEE0_0FFF	DSP Boot ROM		4K
 0xFF60_0000	0xFF6F_FFFF 	DSP CCSR		1M
 0xFF70_0000	0xFF7F_FFFF	PA CCSR			1M
 0xFF80_0000	0xFFFF_FFFF	Boot Page & NAND Buffer 8M

Flashing Images
---------------
To place a new u-boot image in the NAND flash and then boot
with that new image temporarily, use this:
	tftp 1000000 u-boot-nand.bin
	nand erase 0 100000
	nand write 1000000 0 100000
	reset

Using the Device Tree Source File
---------------------------------
To create the DTB (Device Tree Binary) image file,
use a command similar to this:

	dtc -b 0 -f -I dts -O dtb bsc9131rdb.dts > bsc9131rdb.dtb

Likely, that .dts file will come from here;

	linux-2.6/arch/powerpc/boot/dts/bsc9131rdb.dts

Booting Linux
-------------
Place a linux uImage in the TFTP disk area.

	tftp 1000000 uImage
	tftp 2000000 rootfs.ext2.gz.uboot
	tftp c00000 bsc9131rdb.dtb
	bootm 1000000 2000000 c00000
