U-Boot Port to the NS9750 DevKit from NetSilicon

1 Overview
2 Board Configuration
3 Installation


1 Overview
----------

This port supports these NS9750 features.

o one UART

2 Board Configuration
---------------------

Switches:
SW10: 4
SW11: 6,7
SW16: 6,7,8
SW17-SW20: 1
SW4: 3, 6
SW 1: 1
SW2: 4
SW3: 3
SW8: 3 (rotated by 180 degree!!!!)

Serial Console is Port B (bottom right port)

3 Installation
--------------

Have fun,
--
Markus Pietrek <mpietrek@fsforth.de>
